AT-ETX-2iB

Bill of Materials

1. RAD products:

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| ETX-204A\_DTAG/H/AC/OAM/EXT with Ethernet Generator program | 1 | 2 |
| RINGER-2200N | 2 | - |
| RM-34 (for ATE-PIO-USB, ATE-MMUX and ETX204) | 7 | 6 |
| RING-2200-RM | 2 | - |

1. A.T.E. products:

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| ATE-PIO-USB | 1 | 2 |
| ATE-RelayBox/230 | 1 | 2 |
| ATE-MultiMux | 5 | 2 |

1. Cables:
   1. RAD cables:

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| CBL-DB9F-DB9M-STR | 1 | 4 |
| CBL-ETH/STP/STR | 3 | 11 |
| CBL-ETH/STP/STR/3M | 81 | - |
| CBL-MUSB-DB9F | 27 | 2 |

* 1. Specify cables:

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| AT-ETX2iB/CBL01 | 1 | - |
| AT-ETX2iB/CBL02 | 27 | - |
| AT-ETX2iB/CBL03 | 3 | - |
| AT-ETX2iB/CBL04 | 1 | 2 |
| AT-ETX2iB/CBL05 | 2 | 4 |
| AT-ETX2iB/CBL06 | 1 | - |
| AT-ETX2iB/CBL07 | 3 | - |
| AT-ETX2iB/CBL08 | 1 | 2 |

1. Mechanic parts:

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| Masad (width 19”) | 1 (height 32U) | 1 (height 32U) |
| Fixed Shelf | 2 | 2 |
| Removeable shelf | - | 1 |

1. Test equipment
   1. PC’s card

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| Ethernet card | 1 | 1 |

* 1. Movable equipment

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| Barcode scanner | 1 | 1 |
| USB to 4xRS232 | 1 | 2 |
| 10/100 Eth Switch | - | 1 |

1. PC
   1. PC
   2. Screen
   3. Keyboard
   4. Mouse
2. Miscellaneous:

|  |  |  |
| --- | --- | --- |
|  | Mass for 27 units | For 2 separate units |
| 6-way ShortShort power cable 230v | 1 | - |
| 6-way ShortLong power cable 230v | 1 | 2 |
| Extension power cable 230v | 1 | 1 |
| Multiple power socket | 1 | 1 |
| Mouse pad | 1 | 1 |